PCBNEW-BOARD Version 1 date 10/5/2009-14:36:08

$GENERAL
LayerCount 2
Ly 1FFF8001
Links 0
NoConn 0
Di 46925 15914 57851 21086
Ndraw 5
Ntrack 16
Nzone 0
Nmodule 1
Nnets 0
$EndGENERAL

$SHEETDESCR
Sheet A4 11700 8267
Title ""
Date "10 may 2009"
Rev ""
Comp ""
Comment1 ""
Comment2 ""
Comment3 ""
Comment4 ""
$EndSHEETDESCR

$SETUP
InternalUnit 0.000100 INCH
UserGridSize 0.010000 0.010000 mm
ZoneGridSize 250
Layers 2
Layer[0] Rame signal
Layer[15] Componente signal
TrackWidth 50
TrackWidthHistory 50
TrackWidthHistory 170
TrackWidthHistory 400
TrackClearence 60
ZoneClearence 150
DrawSegmWidth 150
EdgeSegmWidth 150
ViaSize 50
ViaDrill 250
ViaSizeHistory 50
ViaSizeHistory 450
MicroViaSize 200
MicroViaDrill 80
MicroViasAllowed 0
TextPcbWidth 120
TextPcbSize 600 800
EdgeModWidth 150
TextModSize 600 600
TextModWidth 120
PadSize 600 600
PadDrill 320
AuxiliaryAxisOrg 0 0
$EndSETUP

$EQUIPOT
Na 0 ""
St ~
$EndEQUIPOT
$MODULE 14dip300
Po 51000 18500 0 15 00200000 4A06DED5 ~~
Li 14dip300
Cd Module Dil 14 pins, pads ronds
Kw DIL
Sc 4A06DED5
AR 
Op 0 0 0
T0 -2000 -500 600 450 0 120 N V 21 "U***"
T1 500 500 600 450 0 120 N V 21 "14DIP300"
DS -4000 -1000 4000 -1000 150 21
DS 4000 1000 -4000 1000 150 21
DS -4000 1000 -4000 -1000 150 21
DS -4000 -500 -3500 -500 150 21
DS -3500 -500 -3500 500 150 21
DS -3500 500 -4000 500 150 21
DS 4000 -1000 4000 1000 150 21
$PAD
Sh "1" R 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -3000 1500
$EndPAD
$PAD
Sh "2" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -2000 1500
$EndPAD
$PAD
Sh "3" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -1000 1500
$EndPAD
$PAD
Sh "4" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 0 1500
$EndPAD
$PAD
Sh "5" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 1000 1500
$EndPAD
$PAD
Sh "6" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 2000 1500
$EndPAD
$PAD
Sh "7" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 3000 1500
$EndPAD
$PAD
Sh "8" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 3000 -1500
$EndPAD
$PAD
Sh "9" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 2000 -1500
$EndPAD
$PAD
Sh "10" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 1000 -1500
$EndPAD
$PAD
Sh "11" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 0 -1500
$EndPAD
$PAD
Sh "12" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -1000 -1500
$EndPAD
$PAD
Sh "13" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -2000 -1500
$EndPAD
$PAD
Sh "14" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -3000 -1500
$EndPAD
$SHAPE3D
Na "dil/dil_14.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  14dip300
$TEXTPCB
Te "10"
Po 60000 18000 600 800 120 0
De 0 0 0 0
$EndTEXTPCB
$TEXTPCB
Te "15"
Po 58650 18700 600 800 120 0
De 0 0 0 0
$EndTEXTPCB
$TEXTPCB
Te "5"
Po 58300 17600 600 800 120 0
De 0 0 0 0
$EndTEXTPCB
$TEXTPCB
Te "40"
Po 62200 18000 600 800 120 0
De 0 0 0 0
$EndTEXTPCB
$TEXTPCB
Te "17/13"
Po 59700 16000 600 800 120 0
De 0 0 0 0
$EndTEXTPCB
$TRACK
Po 0 55300 17800 57650 17800 400 -1
De 0 0 0 0 0
Po 0 55300 18850 57650 18850 400 -1
De 0 0 0 0 0
Po 0 48500 16000 48500 21000 170 -1
De 0 0 0 0 0
Po 0 49500 16000 49500 21000 170 -1
De 0 0 0 0 0
Po 0 50500 16000 50500 21000 170 -1
De 0 0 0 0 0
Po 0 51500 16000 51500 21000 170 -1
De 0 0 0 0 0
Po 0 52500 16000 52500 21000 170 -1
De 0 0 0 0 0
Po 0 53500 16000 53500 21000 170 -1
De 0 0 0 0 0
Po 0 55300 16000 57600 16000 170 -1
De 0 0 0 0 0
Po 0 55300 16300 57600 16300 170 -1
De 0 0 0 0 0
Po 0 55300 17350 57650 17350 400 -1
De 0 0 0 0 0
Po 0 55300 18300 57650 18300 400 -1
De 0 0 0 0 0
Po 0 55200 19650 57750 19650 50 -1
De 0 0 0 0 0
Po 0 55200 19750 57750 19750 50 -1
De 0 0 0 0 0
Po 0 55200 19900 57750 19900 50 -1
De 0 0 0 0 0
Po 0 55200 20100 57750 20100 50 -1
De 0 0 0 0 0
$EndTRACK
$ZONE
$EndZONE
$EndBOARD
